**Pollution treatment by biological Method**

1

Fate of roxarsone during biological nitrogen removal process in wastewater treatment systems  
Chemical Engineering Journal, Volume 255, 1 November 2014, Pages 500-505  
Huan Liu, Guoqing Wang, Jun Ge, Li Liu, Guowei Chen  
[PDF (386 K)](file:///I:\8\1.pdf)  
  
2  
Treatment of Oued El Harrach river water by electrocoagulation noting the effect of the electric field on microorganisms  
Journal of the Taiwan Institute of Chemical Engineers, Volume 45, Issue 4, July 2014, Pages 1564-1570  
N. Boudjema, N. Drouiche, N. Abdi, H. Grib, H. Lounici, A. Pauss, N. Mameri  
[PDF (1724 K)](file:///I:\8\2.pdf)  
3  
  
Upgrading the performances of ultrafiltration membrane system coupled with activated sludge reactor by addition of biofilm supports for the treatment of hospital effluents  
Chemical Engineering Journal, Volume 262, 15 February 2015, Pages 456-463  
Alrhmoun Mousaab, Carrion Claire, Casellas Magali, Dagot Christophe  
[PDF (1803 K)](file:///I:\8\3.pdf)  
  
4  
Preparation of ceramic filler from reusing sewage sludge and application in biological aerated filter for soy protein secondary wastewater treatment  
Journal of Hazardous Materials, In Press, Accepted Manuscript, Available online 23 October 2014  
Suqing Wu, Yuanfeng Qi, Qinyan Yue, Baoyu Gao, Yue Gao, Chunzhen Fan, Shengbing He  
[PDF (487 K)](file:///I:\8\4.pdf)  
  
5  
Effects of Cu exposure on enzyme activities and selection for microbial tolerances during swine-manure composting  
Journal of Hazardous Materials, Volume 283, January 2015, Pages 512-518  
Yanxia Li, Bei Liu, Xuelian Zhang, Min Gao, Jing Wang  
[PDF (683 K)](file:///I:\8\5.pdf)  
6  
  
Effect of redox conditions on pharmaceutical loss during biological wastewater treatment using sequencing batch reactors  
Journal of Hazardous Materials, In Press, Corrected Proof, Available online 12 August 2014  
Lauren B. Stadler, Lijuan Su, Christopher J. Moline, Alexi S. Ernstoff, Diana S. Aga, Nancy G. Love  
[PDF (1588 K)](file:///I:\8\6.pdf)  
  
7  
Combined electrochemical treatment/biological process for the removal of a commercial herbicide solution, U46D®  
Separation and Purification Technology, Volume 132, 20 August 2014, Pages 704-711  
J.-M. Fontmorin, J. Siguié, F. Fourcade, F. Geneste, D. Floner, I. Soutrel, A. Amrane  
[PDF (724 K)](file:///I:\8\7.pdf)  
8  
  
Environmental assessment of nutrient recycling from biological pig slurry treatment – Impact of fertilizer substitution and field emissions  
Bioresource Technology, Volume 163, July 2014, Pages 270-279  
Doris Brockmann, Mary Hanhoun, Ophélie Négri, Arnaud Hélias  
[PDF (1610 K)](file:///I:\8\8.pdf)  
9  
  
Beneficial co-treatment of simple wet flue gas desulphurization wastes with freshwater sewage through development of mixed denitrification–SANI process  
Chemical Engineering Journal, Volume 262, 15 February 2015, Pages 109-118  
Jin Qian, Hui Lu, Feng Jiang, George A. Ekama, Guang-Hao Chen  
[PDF (1712 K)](file:///I:\8\9.pdf)  
  
10  
Prediction model development for petroleum refinery wastewater treatment  
Journal of Water Process Engineering, Volume 4, December 2014, Pages 1-5  
G. Hayder, M.Z. Ramli, M.A. Malek, A. Khamis, N.M. Hilmin  
[PDF (561 K)](file:///I:\8\10.pdf)  
11  
  
Bio-entrapped membrane reactor and salt marsh sediment membrane bioreactor for the treatment of pharmaceutical wastewater: Treatment performance and microbial communities  
Bioresource Technology, Volume 171, November 2014, Pages 265-273  
Kok Kwang Ng, Xueqing Shi, Yinuo Yao, How Yong Ng  
[PDF (1048 K)](file:///I:\8\11.pdf)  
12  
  
Feedback control over the chlorine disinfection process at a wastewater treatment plant using a Smith predictor, a method of characteristics and odometric transformation  
Journal of Environmental Chemical Engineering, Volume 2, Issue 2, June 2014, Pages 1088-1097  
Feridun Demir, Wilbur W. Woo  
[PDF (2801 K)](file:///I:\8\12.pdf)  
  
13  
Effect of salinity on N2O production during shortcut biological nitrogen removal from landfill leachate  
Journal of Bioscience and Bioengineering, Volume 117, Issue 5, May 2014, Pages 582-590  
Mu Liu, Tiantian Liu, Yongzhen Peng, Shuying Wang, Han Xiao  
[PDF (2121 K)](file:///I:\8\13.pdf)  
  
14  
Synthetic textile dyeing wastewater treatment by integration of advanced oxidation and biological processes – Performance analysis with costs reduction  
Journal of Environmental Chemical Engineering, Volume 2, Issue 2, June 2014, Pages 1027-1039  
Carmen S.D. Rodrigues, Luis M. Madeira, Rui A.R. Boaventura  
[PDF (2564 K)](file:///I:\8\14.pdf)  
  
15  
Combined magnetic field and adsorption process for treatment of biologically treated palm oil mill effluent (POME)  
Chemical Engineering Journal, Volume 243, 1 May 2014, Pages 31-42  
Rafie Rushdy Mohammed, Mohammad Reza Ketabchi, Gordon McKay  
[PDF (2846 K)](file:///I:\8\15.pdf)  
  
16  
Power generation and oil sands process-affected water treatment in microbial fuel cells  
Bioresource Technology, Volume 169, October 2014, Pages 581-587  
Jeongdong Choi, Yang Liu  
[PDF (1212 K)](file:///I:\8\16.pdf)  
  
17  
Preparation of clay/alumina and clay/alumina/Ag nanoparticle composites for chemical and bacterial treatment of waste water  
Chemical Engineering Journal, Volume 247, 1 July 2014, Pages 16-24  
B. Yahyaei, S. Azizian, A. Mohammadzadeh, M. Pajohi-Alamoti  
[PDF (1545 K)](file:///I:\8\17.pdf)  
18  
  
Optimization of Two-species Whole-cell Immobilization System Constructed with Marine-derived Fungi and Its Biological Degradation Ability  
Chinese Journal of Chemical Engineering, Volume 22, Issue 2, February 2014, Pages 187-192  
Huiying CHEN, Mingxia WANG, Yubin SHEN, Shanjing YAO  
[PDF (466 K)](file:///I:\8\18.pdf)  
  
19  
Optimisation of coagulation/flocculation for pre-treatment of high strength and saline wastewater: Performance analysis with different coagulant doses  
Chemical Engineering Journal, Volume 254, 15 October 2014, Pages 283-292  
G. Di Bella, M.G. Giustra, G. Freni  
[PDF (1096 K)](file:///I:\8\19.pdf)  
  
20  
Process optimization for the treatment of pharmaceutical wastewater catalyzed by poly sulpha sponge  
Journal of the Taiwan Institute of Chemical Engineers, Volume 45, Issue 4, July 2014, Pages 1739-1747  
Sekar Karthikeyan, Madhava Anil Kumar, Pounsamy Maharaja, Thamodaran Partheeban, Janardhanam Sridevi, Ganesan Sekaran  
[PDF (1224 K)](file:///I:\8\20.pdf)  
21  
  
Sequential anaerobic–aerobic treatment of pharmaceutical wastewater with high salinity  
Bioresource Technology, Volume 153, February 2014, Pages 79-86  
Xueqing Shi, Olivier Lefebvre, Kok Kwang Ng, How Yong Ng  
[PDF (527 K)](file:///I:\8\21.pdf)  
22  
  
Biological permeable reactive barriers coupled with electrokinetic soil flushing for the treatment of diesel-polluted clay soil  
Journal of Hazardous Materials, Volume 283, January 2015, Pages 131-139  
Esperanza Mena, Clara Ruiz, José Villaseñor, Manuel A. Rodrigo, Pablo Cañizares  
[PDF (1129 K)](file:///I:\8\22.pdf)  
23  
  
Performance of a rotating biological contactor treating VOC emissions from paint industry  
Chemical Engineering Journal, Volume 251, 1 September 2014, Pages 269-284  
Aviraj Datta, Ligy Philip  
[PDF (1597 K)](file:///I:\8\23.pdf)  
24  
  
Impact of nutrients supply and pH changes on the elimination of hydrogen sulfide, dimethyl disulfide and ethanethiol by biofiltration  
Chemical Engineering Journal, Volume 258, 15 December 2014, Pages 420-426  
Mouna Ben Jaber, Benoît Anet, Abdeltif Amrane, Catherine Couriol, Thomas Lendormi, Pierre Le Cloirec, Gilles Cogny, Romain Fillières  
[PDF (1006 K)](file:///I:\8\24.pdf)  
  
25  
Assessment of pollution levels resulting from biomass gasification  
Journal of Environmental Chemical Engineering, Volume 2, Issue 3, September 2014, Pages 1228-1235  
E. Menya, J. Olwa, P. Hagström, M. Okure  
[PDF (772 K)](file:///I:\8\25.pdf)  
26  
  
A novel reuse method for waste printed circuit boards as catalyst for wastewater bearing pyridine degradation  
Chemical Engineering Journal, Volume 257, 1 December 2014, Pages 253-261  
Nan Li, Xuebin Lu, Shuting Zhang  
[PDF (1854 K)](file:///I:\8\26.pdf)  
  
27  
Kinetic evaluation of simultaneous COD, ammonia and manganese removal from drinking water using a biological aerated filter system  
Separation and Purification Technology, Volume 130, 10 June 2014, Pages 56-64  
Hassimi Abu Hasan, Siti Rozaimah Sheikh Abdullah, Siti Kartom Kamarudin, Noorhisham Tan Kofli, Nurina Anuar  
[PDF (963 K)](file:///I:\8\27.pdf)  
  
28  
Improvement of biodegradation in compact co-current biotrickling filter by high recycle liquid flow rate: Performance and biodegradation kinetics of ammonia removal  
Process Biochemistry, Volume 49, Issue 10, October 2014, Pages 1733-1740  
Y. Kawase, A. Hirata, T. Kojima, S. Ohmori, H. Akutagawa, K. Uehara, K. Iwata, T. Nakajima, K. Yamamoto  
[PDF (1418 K)](file:///I:\8\28.pdf)  
29  
  
Industrial park wastewater deeply treated and reused by a novel electrochemical oxidation reactor  
Chemical Engineering Journal, Volume 260, 15 January 2015, Pages 427-433  
Runye Zhu, Chuyin Yang, Mingming Zhou, Jiade Wang  
[PDF (1222 K)](file:///I:\8\29.pdf)  
30  
  
Application of response surface method for coagulation process in leachate treatment as pretreatment for Fenton process: Biodegradability improvement  
Journal of Water Process Engineering, Volume 4, December 2014, Pages 67-73  
Mahsa Moradi, Farshid Ghanbari  
[PDF (1523 K)](file:///I:\8\30.pdf)  
31  
  
Fenton and Photo-fenton Oxidation Processes for Degradation of 3-Aminopyridine from Water  
APCBEE Procedia, Volume 9, 2014, Pages 25-29  
Rahul S. Karale, Basavaraju Manu, S. Shrihari  
[PDF (544 K)](file:///I:\8\31.pdf)

32  
A novel application of anaerobic bio-entrapped membrane reactor for the treatment of chemical synthesis-based pharmaceutical wastewater  
Separation and Purification Technology, Volume 132, 20 August 2014, Pages 634-643  
Kok Kwang Ng, Xueqing Shi, Melvin Kai Yin Tang, How Yong Ng  
[PDF (981 K)](file:///I:\8\32.pdf)  
  
33  
Treatment of hypersaline produced water employing a moderately halophilic bacterial consortium in a membrane bioreactor: Effect of salt concentration on organic removal performance, mixed liquor characteristics and membrane fouling  
Bioresource Technology, Volume 164, July 2014, Pages 203-213  
Elham Abdollahzadeh Sharghi, Babak Bonakdarpour, Mehrzad Pakzadeh  
[PDF (765 K)](file:///I:\8\33.pdf)  
  
34  
The effect of COD loading on the granule-based enhanced biological phosphorus removal system and the recoverability  
Bioresource Technology, Volume 171, November 2014, Pages 80-87  
Shenjing Yu, Peide Sun, Wei Zheng, Lujun Chen, Xiongliu Zheng, Jingyi Han, Tao Yan  
[PDF (1967 K)](file:///I:\8\34.pdf)  
35  
  
Optimizing municipal wastewater treatment plants using an improved multi-objective optimization method  
Bioresource Technology, Volume 157, April 2014, Pages 161-165  
Rui Zhang, Wen-Ming Xie, Han-Qing Yu, Wen-Wei Li  
[PDF (852 K)](file:///I:\8\35.pdf)  
  
36  
Combined ozone oxidation and biological aerated filter processes for treatment of cyanide containing electroplating wastewater  
Chemical Engineering Journal, Volume 241, 1 April 2014, Pages 184-189  
Jiaqi Cui, Xiaojun Wang, Yanlei Yuan, Xunwen Guo, Xiaoyang Gu, Lei Jian  
[PDF (620 K)](file:///I:\8\36.pdf)  
  
37  
Validation of linear and non-linear kinetic modeling of saline wastewater treatment by sequencing batch reactor with adapted and non-adapted consortiums  
Desalination, Volume 344, 1 July 2014, Pages 228-235  
Mohammad Mehdi Amin, Mehdi H. Khiadani (Hajian), Ali Fatehizadeh, Ensiyeh Taheri  
[PDF (702 K)](file:///I:\8\37.pdf)  
38  
  
Sertraline accumulation and effects in the estuarine decapod Carcinus maenas: Importance of the history of exposure to chemical stress  
Journal of Hazardous Materials, Volume 283, January 2015, Pages 350-358  
Aurélie P. Rodrigues, Lúcia H.M.L.M. Santos, Maria João Ramalhosa, Cristina Delerue-Matos, Laura Guimarães  
[PDF (1463 K)](file:///I:\8\38.pdf)  
  
39  
Biogas biological desulphurisation under extremely acidic conditions for energetic valorisation in Solid Oxide Fuel Cells  
Chemical Engineering Journal, Volume 255, 1 November 2014, Pages 677-685  
N. de Arespacochaga, C. Valderrama, C. Mesa, L. Bouchy, J.L. Cortina  
[PDF (970 K)](file:///I:\8\39.pdf)  
  
40  
Kinetic characterization of toluene biodegradation by Rhodococcus erythropolis: Towards a rationale for microflora enhancement in bioreactors devoted to air treatment  
Chemical Engineering Journal, Volume 247, 1 July 2014, Pages 199-204  
L. Malhautier, G. Quijano, M. Avezac, J. Rocher, J.L. Fanlo  
[PDF (1015 K)](file:///I:\8\40.pdf)  
  
41  
Biological process for synthesis of semiconductor copper sulfide nanoparticle from mine wastewaters  
Journal of Environmental Chemical Engineering, Volume 2, Issue 1, March 2014, Pages 386-391  
M. Schaffie, M.R. Hosseini  
[PDF (1130 K)](file:///I:\8\41.pdf)  
42  
  
Direct electrochemical oxidation of a pesticide, 2,4-dichlorophenoxyacetic acid, at the surface of a graphite felt electrode: Biodegradability improvement  
Comptes Rendus Chimie, In Press, Corrected Proof, Available online 2 July 2014  
Jean-Marie Fontmorin, Florence Fourcade, Florence Geneste, Isabelle Soutrel, Didier Floner, Abdeltif Amrane  
[PDF (694 K)](file:///I:\8\42.pdf)  
43  
  
Biological Nutrient Removal in a Full Scale Anoxic/Anaerobic/Aerobic/Pre-anoxic-MBR Plant for Low C/N Ratio Municipal Wastewater Treatment  
Chinese Journal of Chemical Engineering, Volume 22, Issue 4, April 2014, Pages 447-454  
Xiang HU, Li XIE, Hojae SHIM, Shanfa ZHANG, Dianhai YANG  
[PDF (567 K)](file:///I:\8\43.pdf)  
44  
  
New insight into the biological treatment by activated sludge: The role of adsorption process  
Bioresource Technology, Volume 153, February 2014, Pages 160-164  
Xiaochun Zhang, Xinrun Li, Qingrui Zhang, Qiuming Peng, Wen Zhang, Faming Gao  
[PDF (1029 K)](file:///I:\8\44.pdf)  
45  
  
A persistent antibiotic partitioning and co-relation with metals in wastewater treatment plant—Chlortetracycline  
Journal of Environmental Chemical Engineering, Volume 2, Issue 3, September 2014, Pages 1596-1603  
R. Puicharla, D.P. Mohapatra, S.K. Brar, P. Drogui, S. Auger, R.Y. Surampalli  
[PDF (556 K)](file:///I:\8\45.pdf)  
  
46  
Identification of some factors affecting pharmaceutical active compounds (PhACs) removal in real wastewater. Case study of fungal treatment of reverse osmosis concentrate  
Journal of Hazardous Materials, In Press, Accepted Manuscript, Available online 14 October 2014  
Marina Badia-Fabregat, Daniel Lucas, Meritxell Gros, Sara Rodríguez-Mozaz, Damià Barceló, Glòria Caminal, Teresa Vicent  
[PDF (304 K)](file:///I:\8\46.pdf)  
  
47  
Application of alga-activated sludge combined system (AASCS) as a novel treatment to remove cephalosporins  
Chemical Engineering Journal, Volume 260, 15 January 2015, Pages 550-556  
Ruixin Guo, Jianqiu Chen  
[PDF (1032 K)](file:///I:\8\47.pdf)  
48  
  
Fenton-biological coupled biochemical oxidation of mixed wastewater for color and COD reduction  
Journal of the Taiwan Institute of Chemical Engineers, Volume 45, Issue 4, July 2014, Pages 1661-1665  
Rabia Nousheen, Aniqa Batool, Muhammad Saif Ur Rehman, Muhammad Asad Ghufran, Malik Tahir Hayat, Tariq Mahmood  
[PDF (768 K)](file:///I:\8\48.pdf)  
  
49  
Physicochemical and porosity characteristics of thermally regenerated activated carbon polluted with biological activated carbon process  
Bioresource Technology, Volume 171, November 2014, Pages 260-264  
Lihua Dong, Wenjun Liu, Renfu Jiang, Zhansheng Wang  
[PDF (427 K)](file:///I:\8\49.pdf)  
  
50  
Colour removal from textile wastewater using a pilot-scale dual-stage MBR and subsequent RO system  
Separation and Purification Technology, Volume 135, 15 October 2014, Pages 135-144  
D. De Jager, M.S. Sheldon, W. Edwards  
[PDF (536 K)](file:///I:\8\50.pdf)  
  
51  
Causal relationships among biological toxicity, geochemical conditions and derived DBPs in groundwater  
Journal of Hazardous Materials, Volume 283, January 2015, Pages 24-34  
Winn-Jung Huang, Yu-Hao Lin, Wei-Yea Chen, Ho-Wen Chen, Ruey-Fang Yu  
[PDF (6586 K)](file:///I:\8\51.pdf)  
  
52  
A forward osmosis membrane system for the post-treatment of MBR-treated landfill leachate  
Journal of Membrane Science, Volume 471, 1 December 2014, Pages 192-200  
Ying Dong, Zhiwei Wang, Chaowei Zhu, Qiaoying Wang, Jixu Tang, Zhichao Wu  
[PDF (1772 K)](file:///I:\8\52.pdf)  
  
53  
A novel recycling process using the treated citric acid wastewater as ingredients water for citric acid production  
Biochemical Engineering Journal, Volume 90, 15 September 2014, Pages 206-213  
Hong-Jian Zhang, Jian-Hua Zhang, Jian Xu, Lei Tang, Zhong-Gui Mao  
[PDF (1202 K)](file:///I:\8\53.pdf)  
  
54  
Xylanase and laccase based enzymatic kraft pulp bleaching reduces adsorbable organic halogen (AOX) in bleach effluents: A pilot scale study  
Bioresource Technology, Volume 169, October 2014, Pages 96-102  
Abha Sharma, Vasanta Vadde Thakur, Anita Shrivastava, Rakesh Kumar Jain, Rajeev Mohan Mathur, Rishi Gupta, Ramesh Chander Kuhad  
[PDF (894 K)](file:///I:\8\54.pdf)  
  
55  
Soft Computing of Biochemical Oxygen Demand Using an Improved T-S Fuzzy Neural Network  
Chinese Journal of Chemical Engineering, In Press, Accepted Manuscript, Available online 18 September 2014  
Junfei Qiao, Wei Li, Honggui Han  
[PDF (370 K)](file:///I:\8\55.pdf)  
  
56  
Startup pattern and performance enhancement of pilot-scale biofilm process for raw water pretreatment  
Bioresource Technology, Volume 172, November 2014, Pages 22-31  
Guang-feng Yang, Li-juan Feng, Qi Yang, Liang Zhu, Jian Xu, Xiang-yang Xu  
[PDF (3499 K)](file:///I:\8\56.pdf)  
57  
  
Nanofiltration as tertiary treatment for the reuse of dairy wastewater treated by membrane bioreactor  
Separation and Purification Technology, Volume 126, 15 April 2014, Pages 21-29  
L.H. Andrade, F.D.S. Mendes, J.C. Espindola, M.C.S. Amaral  
[PDF (848 K)](file:///I:\8\57.pdf)  
  
58  
Treatment of pulp mill wastewater by Cryptococcus podzolicus and solar photo-Fenton: A case study  
Chemical Engineering Journal, Volume 245, 1 June 2014, Pages 158-165  
Lisete Fernandes, Marco S. Lucas, Manuel I. Maldonado, Isabel Oller, Ana Sampaio  
[PDF (851 K)](file:///I:\8\58.pdf)  
59  
  
Organic wastes as carbon sources to promote sulfate reducing bacterial activity for biological remediation of acid mine drainage  
Minerals Engineering, Volume 69, December 2014, Pages 81-90  
Mingliang Zhang, Haixia Wang  
[PDF (1322 K)](file:///I:\8\59.pdf)  
  
60  
Air purification from TCE and PCE contamination in a hybrid bioreactors and biofilter integrated system  
Journal of Hazardous Materials, Volume 264, 15 January 2014, Pages 363-369  
Agnieszka Tabernacka, Ewa Zborowska, Maria Łebkowska, Maciej Borawski  
[PDF (728 K)](file:///I:\8\60.pdf)  
  
61  
Emerging pollutants in the environment: present and future challenges in biomonitoring, ecological risks and bioremediation  
New Biotechnology, In Press, Corrected Proof, Available online 21 January 2014  
Maria Gavrilescu, Kateřina Demnerová, Jens Aamand, Spyros Agathos, Fabio Fava  
[PDF (1419 K)](file:///I:\8\61.pdf)  
62  
  
Aerobic biodegradation of BTEX: Progresses and Prospects  
Journal of Environmental Chemical Engineering, Volume 2, Issue 2, June 2014, Pages 1104-1122  
Muftah H. El-Naas, Janice A. Acio, Ayat E. El Telib  
[PDF (918 K)](file:///I:\8\62.pdf)  
  
63  
Treatment of manufacturing scrap TV boards by nitric acid leaching  
Separation and Purification Technology, Volume 130, 10 June 2014, Pages 151-159  
Ahmet Deniz Bas, Haci Deveci, Ersin Y. Yazici  
[PDF (2064 K)](file:///I:\8\63.pdf)  
  
64  
Experimental analysis and modeling of denitrification using electrocoagulation process  
Separation and Purification Technology, Volume 132, 20 August 2014, Pages 644-654  
T. Yehya, M. Chafi, W. Balla, Ch. Vial, A. Essadki, B. Gourich  
[PDF (1980 K)](file:///I:\8\64.pdf)  
  
65  
Process efficacy and novelty of titania membrane prepared by polymeric sol–gel method in removal of chromium(VI) by surfactant enhanced microfiltration  
Chemical Engineering Journal, Volume 255, 1 November 2014, Pages 483-491  
Suresh M. Doke, Ganapati D. Yadav  
[PDF (2054 K)](file:///I:\8\65.pdf)  
  
66  
Promoting anaerobic biogasification of corn stover through biological pretreatment by liquid fraction of digestate (LFD)  
Bioresource Technology, In Press, Accepted Manuscript, Available online 23 October 2014  
Yun Hu, Yunzhi Pang, Hairong Yuan, Dexun Zou, Yanping Liu, Baoning Zhu, Wachemo Akiber Chufo, Muhammad Jaffar, Xiujin Li  
[PDF (967 K)](file:///I:\8\66.pdf)  
67  
  
Coagulation–flocculation treatment of high-strength agro-industrial wastewater using natural Cassia obtusifolia seed gum: Treatment efficiencies and flocs characterization  
Chemical Engineering Journal, Volume 256, 15 November 2014, Pages 293-305  
Katrina Pui Yee Shak, Ta Yeong Wu  
[PDF (1776 K)](file:///I:\8\67.pdf)  
68  
  
The bacterial communities of bioelectrochemical systems associated with the sulfate removal under different pHs  
Process Biochemistry, Volume 49, Issue 8, August 2014, Pages 1345-1351  
Yue Zheng, Yong Xiao, Zhao-Hui Yang, Song Wu, Hui-Juan Xu, Fang-Yuan Liang, Feng Zhao  
[PDF (2225 K)](file:///I:\8\68.pdf)  
  
69  
Fractality in pH time series of continuous anaerobic bioreactors for tequila vinasses treatment  
Chemical Engineering Science, Volume 109, 19 April 2014, Pages 17-25  
E. Hernandez-Martinez, H. Puebla, H.O. Mendez-Acosta, J. Alvarez-Ramirez  
[PDF (1091 K)](file:///I:\8\69.pdf)  
  
70  
Cleaning strategies for iron-fouled membranes from submerged membrane bioreactor treatment of wastewaters  
Journal of Membrane Science, Volume 475, 1 February 2015, Pages 9-21  
Zhenghua Zhang, Mark W. Bligh, Yuan Wang, Greg L. Leslie, Heriberto Bustamante, T. David Waite  
[PDF (935 K)](file:///I:\8\70.pdf)  
  
71  
Combined adsorbents and reactive oxygen species (ROS) generators in soil for treating reverse osmosis concentrates  
Powder Technology, Volume 264, September 2014, Pages 9-21  
Sung Hee Joo  
[PDF (1622 K)](file:///I:\8\71.pdf)  
72  
  
Bioavailability and biological effect of engineered silver nanoparticles in a forest soil  
Journal of Hazardous Materials, Volume 280, 15 September 2014, Pages 89-96  
S. Carbone, L. Vittori Antisari, F. Gaggia, L. Baffoni, D. Di Gioia, G. Vianello, P. Nannipieri  
[PDF (1260 K)](file:///I:\8\72.pdf)  
  
73  
Recovery of high-value metals from geothermal sites by biosorption and bioaccumulation  
Bioresource Technology, Volume 160, May 2014, Pages 182-190  
Yung-Chung Lo, Chieh-Lun Cheng, Yin-Lung Han, Bor-Yann Chen, Jo-Shu Chang  
[PDF (642 K)](file:///I:\8\73.pdf)  
74  
  
Two phase partitioning membrane bioreactor: A novel biotechnique for the removal of dimethyl sulphide, n-hexane and toluene from waste air  
Chemical Engineering Journal, Volume 256, 15 November 2014, Pages 160-168  
Diëgo Volckaert, Sander Wuytens, Herman Van Langenhove  
[PDF (1785 K)](file:///I:\8\74.pdf)  
75  
  
A comparative study on the performance of different advanced oxidation processes (UV/O3/H2O2) treating linear alkyl benzene (LAB) production plant's wastewater  
Journal of Industrial and Engineering Chemistry, Volume 20, Issue 4, 25 July 2014, Pages 1453-1461  
H. Zangeneh, A.A.L. Zinatizadeh, M. Feizy  
[PDF (2107 K)](file:///I:\8\75.pdf)  
76  
  
Molasses as an efficient low-cost carbon source for biological Cr(VI) removal  
Journal of Hazardous Materials, In Press, Corrected Proof, Available online 13 August 2014  
Michail K. Michailides, Athanasia G. Tekerlekopoulou, Christos S. Akratos, Sandra Coles, Stavros Pavlou, Dimitrios V. Vayenas  
[PDF (1498 K)](file:///I:\8\76.pdf)  
  
77  
Phosphate removal during Fe(II) oxidation in the presence of Cu(II): Characteristics and application for electro-plating wastewater treatment  
Separation and Purification Technology, Volume 132, 20 August 2014, Pages 388-395  
Ting Li, Hongjie Wang, Wenyi Dong, Tongzhou Liu, Feng Ouyang, Qian Zhang  
[PDF (1051 K)](file:///I:\8\77.pdf)  
78  
  
Using central composite experimental design to optimize the degradation of real dye wastewater by Fenton and photo-Fenton reactions  
Dyes and Pigments, Volume 100, January 2014, Pages 184-189  
Francesc Torrades, Julia García-Montaño  
[PDF (552 K)](file:///I:\8\78.pdf)  
  
79  
Kinetics of biological decolorisation of anthraquinone based Reactive Blue 19 using an isolated strain of Enterobacter sp.F NCIM 5545  
Bioresource Technology, Volume 173, December 2014, Pages 342-351  
Chandrakant R. Holkar, Aniruddha B. Pandit, Dipak V. Pinjari  
[PDF (1773 K)](file:///I:\8\79.pdf)  
  
80  
Removal of phenol by acid-washed zero-valent aluminium in the presence of H2O2  
Chemical Engineering Journal, Volume 260, 15 January 2015, Pages 284-290  
Zihang Cheng, Fenglian Fu, Yansong Pang, Bing Tang, Jianwei Lu  
[PDF (1430 K)](file:///I:\8\80.pdf)  
  
81  
Upflow anaerobic sludge blanket-hollow centered packed bed (UASB-HCPB) reactor for thermophilic palm oil mill effluent (POME) treatment  
Biomass and Bioenergy, Volume 67, August 2014, Pages 231-242  
P.E. Poh, M.F. Chong  
[PDF (1961 K)](file:///I:\8\81.pdf)  
  
82  
An anaerobic dynamic membrane bioreactor (AnDMBR) for landfill leachate treatment: Performance and microbial community identification  
Bioresource Technology, Volume 161, June 2014, Pages 29-39  
Zhenfang Xie, Zhiwei Wang, Qiaoying Wang, Chaowei Zhu, Zhichao Wu  
[PDF (1940 K)](file:///I:\8\82.pdf)  
83  
  
Long-term operation of an MBR in the presence of zinc oxide nanoparticles reveals no significant adverse effects on its performance  
Journal of Membrane Science, Volume 471, 1 December 2014, Pages 258-264  
Zhiwei Wang, Fei Huang, Xiaojie Mei, Qiaoying Wang, Hongyang Song, Chaowei Zhu, Zhichao Wu  
[PDF (2245 K)](file:///I:\8\83.pdf)  
84  
  
The impact of ferrous iron/heat-activated persulfate treatment on waste sewage sludge constituents and sorbed antimicrobial micropollutants  
Chemical Engineering Journal, Volume 259, 1 January 2015, Pages 972-980  
Nalan Bilgin Oncu, Nazire Mercan, Isil Akmehmet Balcioglu  
[PDF (783 K)](file:///I:\8\84.pdf)  
85  
  
Detailed treatment line for a specific landfill leachate remediation. Brief economic assessment  
Chemical Engineering Journal, In Press, Corrected Proof, Available online 12 March 2014  
E. De Torres-Socías, L. Prieto-Rodríguez, A. Zapata, I. Fernández-Calderero, I. Oller, S. Malato  
[PDF (436 K)](file:///I:\8\85.pdf)  
86  
  
Investigation of heavy oil refinery wastewater treatment by integrated ozone and activated carbon -supported manganese oxides  
Fuel Processing Technology, Volume 124, August 2014, Pages 165-173  
Chunmao Chen, Lingyong Wei, Xuan Guo, Shaohui Guo, Guangxu Yan  
[PDF (1388 K)](file:///I:\8\86.pdf)  
87  
  
Identification of the salinity effect on N2O production pathway during nitrification: Using stepwise inhibition and 15N isotope labeling methods  
Chemical Engineering Journal, Volume 253, 1 October 2014, Pages 418-426  
Wei Zhao, Yayi Wang, Ximao Lin, Dong Zhou, Mianli Pan, Jian Yang  
[PDF (648 K)](file:///I:\8\81.pdf)  
  
88  
Effect of dissolved oxygen on biological phosphorus removal induced by aerobic/extended-idle regime  
Biochemical Engineering Journal, Volume 90, 15 September 2014, Pages 27-35  
Hongbo Chen, Dongbo Wang, Xiaoming Li, Qi Yang, Kun Luo, Guangming Zeng, Maolin Tang, Weiping Xiong, Guojing Yang  
[PDF (1124 K)](file:///I:\8\88.pdf)  
89  
  
Effect of pH adjustment, solid–liquid separation and chitosan adsorption on pollutants’ removal from pot ale wastewaters  
Journal of Environmental Chemical Engineering, Volume 2, Issue 4, December 2014, Pages 1929-1936  
Davide Dionisi, Sarah Sine Bruce, Malcolm John Barraclough  
[PDF (603 K)](file:///I:\8\89.pdf)  
  
90  
Sulfate reduction at low pH to remediate acid mine drainage  
Journal of Hazardous Materials, Volume 269, 30 March 2014, Pages 98-109  
Irene Sánchez-Andrea, Jose Luis Sanz, Martijn F.M. Bijmans, Alfons J.M. Stams  
[PDF (2100 K)](file:///I:\8\90.pdf)  
  
91  
Anoxic/aerobic granular active carbon assisted MBR integrated with nanofiltration and reverse osmosis for advanced treatment of municipal landfill leachate  
Desalination, Volume 349, 15 September 2014, Pages 136-144  
Guanghui Wang, Zheng Fan, Dexin Wu, Lei Qin, Guoliang Zhang, Congjie Gao, Qin Meng  
[PDF (1231 K)](file:///I:\8\91.pdf)  
92  
  
Recovery of baker’s yeast wastewater with membrane processes for agricultural irrigation purpose: Fouling characterization  
Chemical Engineering Journal, Volume 255, 1 November 2014, Pages 630-640  
Gökhan Balcıoğlu, Z. Beril Gönder  
[PDF (1787 K)](file:///I:\8\92.pdf)  
93  
  
Removal of oil from water using polyurethane foam modified with nanoclay  
Chemical Engineering Journal, Volume 262, 15 February 2015, Pages 278-285  
Amir Ahmad Nikkhah, Hamid Zilouei, Ahmad Asadinezhad, Alireza Keshavarz  
[PDF (1022 K)](file:///I:\8\93.pdf)  
94  
  
Fenton-Anoxic–Oxic/MBR process as a promising process for avermectin fermentation wastewater reclamation  
Separation and Purification Technology, Volume 134, 25 September 2014, Pages 82-89  
Qianhui Xu, Abdalaziz Hamid, Xianghua Wen, Bo Zhang, Ningning Yang  
[PDF (1903 K)](file:///I:\8\94.pdf)  
95  
  
Ammonium removal from anaerobically treated effluent by Chlamydomonas acidophila  
Bioresource Technology, Volume 153, February 2014, Pages 62-68  
Ania Escudero, Fernando Blanco, Arrate Lacalle, Miriam Pinto  
[PDF (905 K)](file:///I:\8\95.pdf)  
  
96  
Effect of hydraulic retention time (HRT) on the anaerobic co-digestion of agro-industrial wastes in a two-stage CSTR system  
Bioresource Technology, Volume 167, September 2014, Pages 407-415  
Margarita Andreas Dareioti, Michael Kornaros  
[PDF (985 K)](file:///I:\8\96.pdf)  
  
97  
Stability of Fe–C micro-electrolysis and biological process in treating ultra-high concentration organic wastewater  
Chemical Engineering Journal, Volume 255, 1 November 2014, Pages 535-540  
Qiushi Zhu, Shaohui Guo, Chunmei Guo, Di Dai, Xinkang Jiao, Tianqi Ma, Jinfu Chen  
[PDF (979 K)](file:///I:\8\97.pdf)  
  
98  
Surface analysis of cobalt-enriched crushed products of spent lithium-ion batteries by X-ray photoelectron spectroscopy  
Separation and Purification Technology, In Press, Accepted Manuscript, Available online 18 October 2014  
Tao Zhang, Yaqun He, Fangfang Wang, Hong Li, Chenlong Duan, Caibin Wu  
[PDF (1025 K)](file:///I:\8\98.pdf)  
  
99  
Indirect electroreduction as pretreatment to enhance biodegradability of metronidazole  
Journal of Hazardous Materials, Volume 278, 15 August 2014, Pages 172-179  
I. Saidi, I. Soutrel, D. Floner, F. Fourcade, N. Bellakhal, A. Amrane, F. Geneste  
[PDF (974 K)](file:///I:\8\99.pdf)  
  
100  
Statistical modeling of photocatalytic degradation of synthetic amoxicillin wastewater (SAW) in an immobilized TiO2 photocatalytic reactor using response surface methodology (RSM)  
Journal of the Taiwan Institute of Chemical Engineers, Volume 45, Issue 4, July 2014, Pages 1717-1726  
Z.M. Shaykhi, A.A.L. Zinatizadeh  
[PDF (3376 K)](file:///I:\8\100.pdf)